|  |  |
| --- | --- |
| **Millersburg Water Company - Consumer Confidence Report Amendment**  **IN5220015**  The following results are the correct detections within your drinking water. |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Lead and Copper** | Date Sampled | 90th Percentile | Units | Likely Source of Contamination |
|  |  |  |  |  |
| **Copper** | 09/13/2018 | 0.43 | ppm | Erosion of natural deposits; Leaching from wood preservatives; Corrosion of household plumbing systems. |

**Regulated Contaminants**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Disinfectants and Disinfection By-Products** | Collection Date | Highest Level Detected | Range of Levels Detected | Units | Likely Source of Contamination |
|  |  |  |  |  |  |
| **Chlorine** | 2020 | 1 | 1 - 1 | ppm | Water additive used to control microbes. |
|  |  |  |  |  |  |
| **Haloacetic Acids (HAA5)** | 2020 | 8 | 7.6 - 7.6 | ppb | By-product of drinking water disinfection. |
|  |  |  |  |  |  |
| **Total Trihalomethanes (TTHM)** | 2020 | 43 | 42.9 - 42.9 | ppb | By-product of drinking water disinfection. |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
| **Nitrate [measured as Nitrogen]** | 2020 | 2 | 0.2 - 4.2 | ppm | Runoff from fertilizer use; Leaching from septic tanks, sewage; Erosion of natural deposits. |
|  |  |  |  |  |  |
| **Radioactive Contaminants** | Collection Date | Highest Level Detected | Range of Levels Detected | Units | Likely Source of Contamination |
|  |  |  |  |  |  |
| **Combined Radium 226/228** | 2020 | 0.46 | 0.46 - 0.46 | pCi/L | Erosion of natural deposits. |

**If you have any questions, please contact Ben Eldridge 574-971-6429**